# configuration file generated by Bochs
plugin_ctrl: unmapped=1, biosdev=1, speaker=1, extfpuirq=1, parallel=1, serial=1, gameport=1
config_interface: win32config
display_library: win32
memory: host=64, guest=64
romimage: file="./BIOS-bochs-latest"
vgaromimage: file="./VGABIOS-lgpl-latest"
# vgaromimage: file="./VGABIOS-lgpl-latest-cirrus-debug"
boot: floppy
floppy_bootsig_check: disabled=0
floppya: type=1_44, 1_44="..\cf2023.img", status=inserted
# no floppyb
ata0: enabled=1, ioaddr1=0x1f0, ioaddr2=0x3f0, irq=14
ata1: enabled=1, ioaddr1=0x170, ioaddr2=0x370, irq=15
ata2: enabled=0
ata3: enabled=0
pci: enabled=1, chipset=i440fx
vga: extension=vbe, update_freq=5
cpu: model=p4_willamette, count=1, ips=50000000, reset_on_triple_fault=1, ignore_bad_msrs=1, msrs="msrs.def", cpuid_limit_winnt=0
cpuid: x86_64=1, mmx=1, sep=1, simd=sse4_2, apic=xapic, aes=1, movbe=1, xsave=1
cpuid: family=6, model=0x1a, stepping=5
print_timestamps: enabled=0
port_e9_hack: enabled=0
private_colormap: enabled=0
clock: sync=none, time0=local, rtc_sync=0
# no cmosimage
# no loader
log: -
logprefix: %t%e%d
panic: action=ask
error: action=report
info: action=report
debug: action=ignore
keyboard: type=mf, serial_delay=250, paste_delay=100000, keymap=, user_shortcut=
mouse: enabled=0, type=ps2, toggle=ctrl+mbutton
parport1: enabled=1, file=""
parport2: enabled=0
com1: enabled=1, mode=null, dev=""
com2: enabled=0
com3: enabled=0
com4: enabled=0
